**Intelligent Paste Strength Tester**



**Application**

It is suitable for the testing of the pulling force of the rivets, the bonding strength of the wall insulation materials and the bonding strength of the exterior wall facing bricks, all kinds of plates and paints.

**Feature**

1. Light alloy body, s-type tension sensor, high precision.
2. Embedded digital tension meter.
3. With clear, peak, storage, backlight and other functions.
4. Ultra-low power design, no operation automatic shutdown, continuous working time can exceed 200 hours.
5. Two measurement modes: strength (MPa) and force value (KN).

**Technical Parameter**

|  |  |  |
| --- | --- | --- |
| Item | GTJ-2000A | GTJ-6000C |
| Instrument structure | Split | Integrated |
| Measuring range | 0-6.000kN/3.75Mpa | |
| Display mode | kN/Mpa adjustable | |
| Resolution | 0.001kN | |
| Hollow oil cylinder stroke | 10mm | |
| Data storage | 500 | |
| Data query and deletion | yes | |
| Peak hold function | yes | |
| Night lighting function | yes | |
| Polyline correction | 10 steps | |
| Body material weight | Stainless steel material 4.5kg | Alloy materials 2.0kg |