**LOVELY-Vx Micro pull-out anchor tester**

**USAGE OVERVIEW**

LOVELY-Vx Micro pull-out anchor tester is mainly used to detect, ∮6-∮12 masonry structure steel bar planting bar, M6-M12 expansion bolt, chemical anchor bolt, and various anchors' pull-out resistance. The on-site anti-pulling force test (test) of glass curtain wall is a necessary testing instrument for each (quality inspection unit, reinforcement unit, supervision unit, university, etc.).

**PRODUCT FEATURES**

1.Light weight. 2.6kg oil cylinder, 2.8kg smaller manual pump.2.200 data records, query, LCD lighting function.3.Peak hold, less than 4% unloading in 2 minutes, automatic shutdown without operation.4.The 10-segment polyline correction of the value improves the accuracy of the instrument.5.The power supply is a high-capacity rechargeable lithium battery and ultra-low power consumption design, and the continuous working time can exceed 200 hours.6.Using imported seals, durable.7.Corrosion-resistant electrostatic spraying on the surface of hydraulic cylinder, nickel-plated piston and sliding sleeve.8.Overload protection structure is adopted, and the cylinder will not be damaged if it exceeds the range, so it can be used safely.

**TECHNICAL PARAMETERS**